Lab 2.

A virtual wire interface binds two Ethernet ports together. A virtual wire interface allows all traffic or just selected VLAN traffic to pass between the ports. No other switching or routing services are available.

The firewall requires a virtual router to obtain routes to other subnets either using static routes that you manually define, or through participation in Layer 3 routing protocols that provide dynamic routes