Checklist:

* Internal e1/2 172.20.240.254/24
* User e1/4 172.20.242.254/24
* Public, e1/1 172.20.241.254/24
* MgtInt 172.20.242.150

configure

set deviceconfig system ip-address 172.20.242.150

commit

show system services

set deviceconfig system service disable <name>

commit

set deviceconfig system permitted-ip 172.20.242.100  
commit

set mgt-config users admin password

commit

exit

show admins all

delete mgt-config users <username>

Device -> Licenses

Device -> Dynamic Updates

Device -> Setup -> Management -> General Settingds